|  |  |
| --- | --- |
| **QUESTION** | **Application** |
| **NS11.1** | Are Pile Driving Operations applied as required? |
| **SPECs, 13-4.03C(1) General** | Minimize or eliminate discharge of material into the air, storm drain systems, and receiving waters while taking delivery of, using, or storing the following materials:  6. Petroleum materials, including fuel, oil, and grease |
| **CGP, Attachment C.C.1; D.C.1; E.C.1** | Risk Level 1, 2 and 3 dischargers shall implement measures to control all non-storm water discharges during construction. |
| **LTP VIII.** | Dischargers shall minimize or prevent pollutants in authorized non-storm water discharges through the use of controls, structures and management practices that achieve BAT for toxic and non-conventional pollutants and BCT for conventional pollutants |

|  |  |
| --- | --- |
|  | **Implementation** |
| **NS11.2** | Are Pile Driving Operations implemented properly? |
| **SPECs, 13-4.03C(1) General** | The following activities must be performed at least 100 feet from concentrated flows of stormwater, drainage courses, and inlets if within the floodplain and at least 50 feet if outside the floodplain, unless otherwise authorized:  2. Storing pile-driving equipment... |
| **SPECs, 13-4.03E(9) Pile Driving** | Keep spill kits and cleanup materials at pile driving locations. Park pile driving equipment over drip pans, absorbent pads, or plastic sheeting with absorbent material. Protect pile driving equipment by parking on plywood and covering with plastic whenever precipitation is forecasted.  Store pile driving equipment on level ground and protect it from stormwater run-on when not in use. Use vegetable oil instead of hydraulic fluid if practicable. |
| **CGP, Order IV.E Proper Operation and Maintenance** | The discharger shall at all times properly operate and maintain any facilities and systems of treatment and control (and related appurtenances) which are installed or used by the discharger to achieve compliance with the conditions of this General Permit. Proper operation and maintenance also includes adequate laboratory controls and appropriate quality assurance procedures. Proper operation and maintenance may require the operation of backup or auxiliary facilities or similar systems installed by a discharger when necessary to achieve compliance with the conditions of this General Permit. |