|  |  |
| --- | --- |
| **QUESTION** | **Application** |
| **NS12.1** | Are Concrete Curing practices applied as required? |
| **SPECs, 13-4.03C(1) General** | Minimize or eliminate discharge of material into the air, storm drain systems, and receiving waters while taking delivery of, using, or storing the following materials:  1. Hazardous chemicals, including acids, lime, glues, adhesives, paints, solvents, and curing compounds |
| **CGP, Attachment C.C.1; D.C.1; E.C.1** | Risk Level 1, 2 and 3 dischargers shall implement measures to control all non-storm water discharges during construction. |
| **LTP VIII.** | Dischargers shall minimize or prevent pollutants in authorized non-storm water discharges through the use of controls, structures and management practices that achieve BAT for toxic and non-conventional pollutants and BCT for conventional pollutants |

|  |  |
| --- | --- |
|  | **Implementation** |
| **NS12.2** | Are Concrete Curing practices implemented properly? |
| **SPECs, 13-4.03E(10) Concrete Curing** | Do not overspray chemical curing compounds. Minimize the drift by spraying as close to the concrete as practicable. Do not allow runoff of curing compounds. Cover drainage inlets before applying the curing compound.  Minimize the use and discharge of water by using wet blankets or similar methods to maintain moisture when concrete is curing. |
| **CGP, Order IV.E Proper Operation and maintenance** | The discharger shall at all times properly operate and maintain any facilities and systems of treatment and control (and related appurtenances) which are installed or used by the discharger to achieve compliance with the conditions of this General Permit. Proper operation and maintenance also includes adequate laboratory controls and appropriate quality assurance procedures. Proper operation and maintenance may require the operation of backup or auxiliary facilities or similar systems installed by a discharger when necessary to achieve compliance with the conditions of this General Permit. |